# TTP Detail – T1599.001

## TTP Information

Name: Network Address Translation Traversal

Description: Adversaries may bridge network boundaries by modifying a network device’s Network Address Translation (NAT) configuration. Malicious modifications to NAT may enable an adversary to bypass restrictions on traffic routing that otherwise separate trusted and untrusted networks.  
  
Network devices such as routers and firewalls that connect multiple networks together may implement NAT during the process of passing packets between networks. When performing NAT, the network device will rewrite the source and/or destination addresses of the IP address header. Some network designs require NAT for the packets to cross the border device. A typical example of this is environments where internal networks make use of non-Internet routable addresses.(Citation: RFC1918)  
  
When an adversary gains control of a network boundary device, they can either leverage existing NAT configurations to send traffic between two separated networks, or they can implement NAT configurations of their own design. In the case of network designs that require NAT to function, this enables the adversary to overcome inherent routing limitations that would normally prevent them from accessing protected systems behind the border device. In the case of network designs that do not require NAT, address translation can be used by adversaries to obscure their activities, as changing the addresses of packets that traverse a network boundary device can make monitoring data transmissions more challenging for defenders.   
  
Adversaries may use [Patch System Image](https://attack.mitre.org/techniques/T1601/001) to change the operating system of a network device, implementing their own custom NAT mechanisms to further obscure their activities

## Threat-Mapped Scoring

Score: 1.8

Priority: P4 - Informational (Low)

## Kill Chain Phases

**•** mitre-attack: defense-evasion