# CWE Detail – CWE-198

## Description

The product receives input from an upstream component, but it does not account for byte ordering (e.g. big-endian and little-endian) when processing the input, causing an incorrect number or value to be used.

## Extended Description

N/A

## Threat-Mapped Scoring

Score: 0.0

Priority: Unclassified

## Modes of Introduction

**•** Implementation: N/A

## Common Consequences

**•** Impact: Unexpected State — Notes:

## Applicable Platforms

**•** None (Class: Not Language-Specific, Prevalence: Undetermined)

## Notes

**•** Research Gap: Under-reported.